                                                                      Date:    August 19, 1995 Sheet     1 of     1

                                                                      Size Document Number REV

                                                                        A A

                                                                      Title

                                                                         Amperite #6-4 ballast tube replacement

               C1
               0.1

            VCC

      R1
      100k
      1/8W

   VCC

                   3

                   2

                            1

                      8

                      4

                        U1A
                        LM358

                     VCC

                              VR1
                              100k

                           current adj.
                                                                       Q1
                                                                       TIP31

                                                     5

                                                     6

                                                              7

                                                        8

                                                        4

                                                          U1B
                                                          LM358

                                                       VCC

                                                                   VCC

                                                                                  C

                                                                            Q1

                                                                                B C E

                                                                      R2
                                                                      1
                                                                      2W

     4

     8

       D1
       LM385-1.2

n/c

   D1 (bottom)
          A VCC

                                                   P1
                                                   Octal tube base

      C

                                                                            Replacement for Amperite type #6-4
                                                                            ballast tube as used as R-32 in
                                                                            AF Amplifier AM-65/GRC
                                                                            (Fed Tele & Rad part/dwg #GH-2677-2)

                                                                            Note: Ground as shown here is for

                                                                            Adjust VR1 for 600 mA through circuit
                                                                            at 6.3 VDC

                                                                            reference only; in normal use,
                                                                            the ground net will float at roughly
                                                                            6.3V above chassis ground.

                                                                            Unless otherwise specified:
                                                                            1. Resistances are in ohms
                                                                            2. Capacitances are in microfarads